**Overview**

A rugged tab with integrated STQC certified Finger Print Sensor and 2” Thermal Printer. It is available in Android OS and comes with SDK for FPS and printer that helps in rapid deployment of custom applications. With in-built features like 7” display, GPS/GLONASS for location tracking, 5MP Auto focus camera and wireless features like 3G/4G, Bluetooth and Wifi, the terminal can be deployed anywhere in the field.

**Features**

* Compact and Rugged
* High speed Quad Core Processor @1.3GHz
* Android Operating System
* 7” 1280x720 TFT Display with Touch Panel
* Inbuilt 5MP Auto focus camera, Network 3G/4G and LED Flash
* Integrated 2” Thermal Printer, additional battery and STQC certified FPS

**Application Areas**

* Authentication applications
* Time & attendance applications
* Banking/ Micro Finance
* Billing/ Delivery services
* Customized applications

**Technical Specifications**

|  |  |  |  |
| --- | --- | --- | --- |
|  | Processor | CPU | High Speed Quad Core |
| Speed | 1.3GHz |
| C:\Users\Aamani\Downloads\2-OperatingSystem.png | Operating System | OS | Android |
| C:\Users\Aamani\Downloads\3-Memory.png | Memory | RAM | 2GB |
| Internal Memory | 16GB |
| External Memory | Up to 128GB memory card |
| C:\Users\Aamani\Downloads\4-CommunicationPort.png | Communication Ports | USB | Micro USB 2.0 |
| OTG | Yes |
| C:\Users\Aamani\Downloads\5-Wireless.png | Wireless Connectivity | WLAN | Yes |
| Connectivity | 3G/4G |
| Bluetooth | Yes |
| C:\Users\Aamani\Downloads\6-Power.png | Power | In-built Battery | 3500mAh |
| Additional battery | Rechargeable Li-Ion 2600mAh |
| C:\Users\Aamani\Downloads\7-DisplayKeypad.png | Display & Keypad | Display type & size | 7” 1280x720 TFT w/Touch Panel |
| C:\Users\Aamani\Downloads\8-Optional.png | Other Peripherals | Camera | 5MP Auto Focus (Rear) |
| Location | GPS, GLONASS |
| SIM | Dual SIM |
| Sound | 3.5mm ear jack |
| C:\Users\Aamani\Downloads\9-Dimensions.png | Dimensions | H x W x D in mm | 248 x 114 x 40/65 |
| C:\Users\Aamani\Downloads\10-Operating.png | Operating Conditions | Operating Temperature | 0°C - 50°C |
| Relative Humidity | 5-95% (Non-condensing) |